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TENDER NOTICE: Rehabilitation of 2 health facilities - Galdogob District- Mudug Region, Puntland Somalia.

Date of EoI: 			10th Oct 2026
Closing date: 			23th Oct 2026
Project Ref No:		CBPF-SOM-26-S-NGO-40422
To be addressed to:		NODO Garowe Office
Contact address:                   Behind Kallis Cafeteria, Lascanood road. 
Contact person:		Maryam Abdinasir, Phone number: +252906279042
Service Delivery Period:      14 days

As one of the multi-sectoral local organizations in Somalia, Nomadic Development Organization (NODO) help vulnerable communities in distress and turn their crisis to opportunities and self-reliance. We help communities recover from disaster, build resilient communities, strengthen their capacity to with stand sudden shocks and find their own solutions.
NODO works in emergency response programs Including Health, WASH, Nutrition, Education in Emergency (EIE) and Resilience programs including climate change adaptation and Environmental conservation among others. We help internally displaced women and girls access safe spaces and dignified case managements.
Nomadic Development Organization (NODO) is implementing an integrated Health and Nutrition project titled ‘Provision of Integrated Lifesaving Health and Nutrition Assistance to Support Underserved Communities Impacted by Climatic Shocks in Galdogob District, Somalia’ with the fund of Somalia Humanitarian Fund (SHF).  For this purpose, NODO is inviting to bid for the the Rehabilitation of two static facilities in Galdogob district by a capable vendor selected through a competitive tendering process and NODO H&N officer/Project Coordinator will supervise the quality of the contents of the Rehabilitation of the two static facilities as per the advert.
NODO hereby invites applications to establish contract with reputable and financially stable vendors with vast experience and capable of Rehabilitation works in the targeted Galdogob district as specified in the bid advert that will be implemented from 25th Oct 2026 to 14th Nov 2026. The vendors with capacities and can fulfil the required qualifications will be required to submit their expression of interest and the BoQ template filled out to NODO Garowe office before the closing dates as stated above:
B.3 BoQ Rehabilitation of HFs
BOQS TYPICAL TWO TWIN BLOCK VIP LATRINEs & INSTALLATION of HAND-WASHING FACILITIES - FOR  HCs
	Item No
	DESCRIPTION
	UNIT
	QUANTITY
	RATE (USD)
	AMOUNT (USD)

	1
	Excavation
	 
	 
	 
	 

	1.1
	Prepare site by stripping top 200 mm of soil to remove all debris including sand (if any) from site and carting away spoil
	m2
	              30 
	 
	$0.00

	1.2
	Excavate for foundation strip commencing at stripped levels depth not exceeding 1.50m deep
	m3
	              15 
	 
	$0.00

	1.3
	Pit excavation commencing at stripped levels depth not exceeding 1.50m deep
	m3
	              13 
	 
	$0.00

	1.4
	Extra-over for excavation in rock
	m3
	                2 
	 
	$0.00

	1.5
	Remove surplus excavated material from site
	m3
	              16 
	 
	$0.00

	1.6
	Backfill around foundation
	m3
	              14 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	2
	Filing
	 
	 
	 
	 

	2.1
	300 mm thick approved hardcore filling spread, well rammed and compacted in 150mm layers to receive concrete surface bed 
	m3
	                4 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	3
	Concrete work
	 
	 
	 
	 

	3.1
	100mm thick floor slab with surface steel trowelled smooth
	m2
	              21 
	 
	$0.00

	3.2
	Allow for pit/squat hole in 100mm thick floor slab
	No
	                2 
	 
	$0.00

	3.3
	Formwork to edges of strip footing girth over 75mm but not exceeding 150mm 
	m
	              62 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	4
	Walling
	 
	 
	 
	 

	4.1
	300mm Thick rubble stone foundation walling in cement and sand mortar (1:3)
	m2
	              23 
	 
	$0.00

	4.2
	150mm thick masonry wall
	m2
	                5 
	 
	$0.00

	4.3
	One layer 1000gauge polythene sheet damp proof membrane under beds: 300mm laps
	m2
	              21 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	5
	SUPERSTRUCTURES
	 
	 
	 
	 

	5.1
	Walling
	 
	 
	 
	 

	5.2
	150 Thick load bearing solid concrete block walling 
	m2
	              49 
	 
	$0.00

	5.3
	Precast concrete 600 x 300 x 50 mm Thick twice weathered and throated coping jointed and pointed in cement and sand mortar
	m
	                7 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	6
	Roof Structure
	 
	 
	 
	 

	6.1
	200mm x 15mm Fascia Board
	m
	              14 
	 
	$0.00

	6.2
	l00x50mmRafters
	m
	              11 
	 
	$0.00

	6.3
	100mm x 50mm wall plate
	m
	              12 
	 
	$0.00

	6.4
	50 x 50 Purlins
	m
	              13 
	 
	$0.00

	6.5
	30 Gauge galvanized corrugated iron sheets fixed to timber Purlins
	m2
	              12 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	7
	Painting and Decorating
	 
	 
	 
	 

	7.1
	Knot prime stop and apply two undercoats and one gloss finishing coat oil paint to fascia board 200- 300 mm wide
	m
	              14 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	8
	Doors 
	 
	 
	 
	 

	8.1
	45mm thick Match boarded timber double door, overall size 900x 2100mm high
	No
	                2 
	 
	$0.00

	8.2
	150x50mm frame two labours plugged screwed and pellated
	m
	              10 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	8.3
	Supply and fix the following ironmongery to timber with matching screws
	 
	 
	 
	 

	8.4
	hinges
	Pairs
	3.0
	 
	$0.00

	8.5
	Three lever mortice lock
	No
	                2 
	 
	$0.00

	8.6
	Rubber door stop
	No
	                2 
	 
	$0.00

	8.7
	Prepare and apply two undercoats and one finishing coat oil paint to timber door
	m2
	                8 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	9
	Floor Finishes
	 
	 
	 
	 

	9.1
	Cement and sand mortar (1:4)trowelled beds: on concrete: to
	 
	 
	 
	 

	9.2
	Non slip approved ceramic floor tiles size 300x300x8mm thick as approved by the Engineer: bedded on cement and sand screeds(measured separately) : jointed and grouted in matching colour cement mortar
	 
	 
	 
	 

	9.3
	100 x 25mm Thick skirting to junction with floor and wall finish
	m
	              19 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$57.00

	10
	Wall Finishes
	 
	 
	 
	 

	10.1
	Walls internally (Optional)
	m2
	              48 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	10.2
	12mm lime plaster: steel trowelled finish: on concrete, block work or stonework: to
	 
	 
	 
	 

	10.3
	Walls externally and internally 
	m2
	              40 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	11
	Prepare and apply three coats plastic emulsion paint to:
	 
	 
	 
	 

	11.1
	Supply and fix hand washing concrete basin size 300mm x 450mm
	No
	                1 
	 
	$0.00

	11.2
	Pit/squat hole cover
	No
	                2 
	 
	$0.00

	11.3
	100mm diameter PVC vent pipe with fly screen top
	m
	                5 
	 
	$0.00

	11.4
	150mm diameter PVC pipe inclined at 45 degrees
	m
	                2 
	 
	$0.00

	 
	Sub-total
	 
	 
	 
	$0.00

	 
	Total cost estimate of typical a single twin-block VIP latrines 
	 
	 
	 
	$0.00

	 
	Total cost twin-block VIP latrines for 2 HCs 
	 
	 
	 
	$0.00

	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	 
	Minor repair of Hand-Washing Facilities and Sanitation facilities
	 
	 
	 
	 

	Item No
	DESCRIPTION
	UNIT
	QUANTITY
	RATE (USD)
	AMOUNT (USD)

	1
	Procurement and installation of new handwashing stations for Health centers and PHUs o
	m³
	12
	 
	$0.00

	2
	Minor repair and maintenance of Handwashing stations 
	LS
	10
	 
	$0.00

	3
	Maintenance and minor repair ofexisitng latrines
	LS
	10
	 
	$0.00

	 
	Total Cost Hand-washing Facilities & Desludging Services
	 
	 
	 
	 $         -   

	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	 
	Summary Total Cost
	 
	 
	 
	 

	 
	Total cost for Twin-Block Latrines for HCs
	 
	 
	 
	$0.00

	 
	Total Cost Hand-washing Facilities
	 
	 
	 
	 $         -   

	 
	Main total for HCs Latrines, Hand-washing Facilities and Desludging Services
	 $         -   

	 
	Health Center BOQs for Construction of Incinerator, Sharp, Ash & Placenta Pits
	 
	 
	 
	 

	Item No
	Description
	Unit
	Qty
	Rate
	Amount

	A
	 SUBSTRUCTURES 
	 
	 
	 
	 

	1
	Earth Works
	 
	 
	 
	 

	1.1
	cart away the spoil material in a place recommended by the engineeer hose usable materials must be dismantled carefully and return back to the client however if the contractor failed to do that he will purchase a new one or an equivalent amount of payment will be deducted.
	LS
	1
	 
	0

	1.2
	Excavate for strip footing not less than 500mm deep, starting from stripped levels( not exceeding 400mm width)
	m³
	1.5
	 
	0

	 
	 Total Carried 
	 
	 
	 
	 $         -   

	B
	 SUPER STRUCTURES 
	 
	 
	 
	 

	2
	 Walling
	 
	 
	 
	 

	 
	Approved fire clay bricks  or other equal and approved to the inner walls of the incinerator; bedded and jointed in (1:3) cement and sand mortar and reinforced with hoop iron every alternate course 
	 
	 
	 
	 

	2.1
	200mm thick walling externally
	m²
	22.5
	 
	0

	 
	 Total Carried 
	 
	 
	 
	 $         -   

	3
	Concrete Works
	 
	 
	 
	 

	 
	Reinforced concrete in class C-30 (with a 28-day 150mm cube crushing strength of 30MPa), cast into formworks and vibrated around rod reinforcement bars.
	 
	 
	 
	 

	3.1
	final beams and cover slap, this also includes columns of the entire roof and flooring
	m³
	1.36
	 
	0

	 
	 Total Carried 
	 
	 
	 
	 $         -   

	4
	 Finishes
	 
	 
	 
	 

	 
	Plastering
	 
	 
	 
	 

	 
	20mm thick cement/sand (1:5) plaster as described to:
	 
	 
	 
	 

	4.1
	External and iternal Walls
	m²
	45
	 
	            -   

	 
	Painting
	 
	 
	 
	 

	 
	Prepare the surface and apply three coats of plastic emulsion paint of chosen type and color to :
	 
	 
	 
	 

	4.2
	Plastered walls(external and internal walls)
	m²
	45
	 
	            -   

	 
	 Total Carried 
	 
	 
	 
	 $         -   

	5
	Doors
	 
	 
	 
	 

	5.1
	Provide and install steel door size( 1000mm*1000mm) price of the work shall include door lock, handles, hinges and accessors and installation of incinerator chimney of 4.5m( Allamunium type)
	item
	1
	 
	            -   

	 
	 Total Carried 
	 
	 
	 
	 $         -   

	6
	Roofing for the entire hall(5*5m)
	 
	 
	 
	 

	6.1
	Supply and fix complete roof structure of the ward regarding following specifications; a. providing and fixing roof framing in trussess b: providing and fixing G-28 galvanized roof sheet, the job shall include all the necessary materials to comlete the roof structure
	m²
	44
	 
	            -   

	 
	 Total Carried 
	 
	 
	 
	 $         -   

	 
	 Total Budget for construction of one Incinerator 
	 
	 
	 
	 $         -   

	 
	 
	 
	 
	 
	 

	BOQ's for construction of Placenta Pits for Health Centers 

	Item
	Description
	Unit 
	Quantity
	Rate (USD)
	Amount (USD)

	A
	Site Preperation & Earth Work Excavation
	 
	 
	 
	 

	1.1
	Cleaning and removal of trees/shrubs
	LS
	1
	 
	0

	1.2
	Earth work excavation of ash pit (length 2.5m x width 1.5m x depth 1.5m)
	m³
	26
	 
	 

	1.3
	Extra-over for excavation in rock
	m³
	1
	 
	0

	1.4
	Remove surplus excavated material from site and backfill around foundation
	m³
	4
	 
	0

	 
	Total Carried
	 
	 
	 
	 $         -   

	 
	Placenta Pit Walls Construction and Concrete Slabs
	 
	 
	 
	 

	2
	Construct stone masonry wall for lining the walls of the pit to prevent the walls from collapsing including plastering
	m³
	26
	 
	0

	3
	concrete slab (2.5mx2mx0.2m) at the basement of the pit to avoid leaching at the groundwater
	m³
	4
	 
	0

	4
	concrete water-tight  cover slab at the top of the pit 50cm above the ground to avoid flood runoff water, leaving space for the lockable hatch (50cmx40cm) and space for installation of vent pipe (circular 40mm-50mm) 
	m³
	6
	 
	0

	5
	Concrete lockable access hatch (50cmx40cmx10cm)
	Pcs
	1
	 
	0

	6
	Ventilation pipe (40mm-50mm diameter and height 3.5m) with rain cover
	Pcs
	1
	 
	0

	 
	Total Carried
	 
	 
	 
	 $         -   

	 
	Total 1 Placenta pit
	 
	 
	 
	 $         -   

	 
	 
	 
	 
	 
	 

	 
	BOQ's for construction of Ash Pit for  HCs(length 2.5m x width 1.5m x depth 1.5m)
	 
	 
	 
	 

	Item
	Description
	Unit 
	Quantity
	Rate (USD)
	Amount (USD)

	A
	Site Preperation & Earth Work Excavation
	 
	 
	 
	 

	1.1
	Cleaning and removal of trees/shrubs
	LS
	1
	 
	0

	1.2
	Earth work excavation of ash pit (length 2.5m x width 1.5m x depth 1.5m)
	m³
	24
	 
	0

	1.3
	Extra-over for excavation in rock
	m³
	1
	 
	0

	1.4
	Remove surplus excavated material from site and backfill around foundation
	m³
	4
	 
	0

	 
	Total Carried
	 
	 
	 
	 $         -   

	B
	Ash Pit Walls Construction and Concrete Slabs
	 
	 
	 
	 

	2.1
	Construct and install ash pit walls lining with stone masonry to prevent the walls from collapsing  (length 2.5m x width 1.5m x depth 1.5m)
	m³
	26
	 
	0

	2.2
	Construct and install concrete slab at the basement of the ash pit to avoid leaching at the groundwater (length 2.5m x width 1m x breadth 0.2m)
	m³
	4
	 
	0

	2.3
	Construct and install concrete water-tight  cover slab at the top of the pit above the ground to avoid flood runoff water (length 2.2m x width 0.8m x breadth 0.1m), leaving space for the concrete cover lid (0.6m x 0.4m)
	m³
	6
	 
	0

	2.4
	Construct and install concrete cover lid (06m x 0.4m x 0.1m)
	m²
	1
	 
	0

	 
	Total Carried
	 
	 
	 
	 $         -   

	 
	Total for Construction one Ash Pit
	1
	 
	 
	 $         -   

	 
	 
	 
	 
	 
	 

	 
	BOQ's for construction of Sharp Pit for  HCs(length 2.5m x width 1.5m x depth 1.5m)
	 
	 
	 
	 

	Item
	Description
	Unit 
	Quantity
	Rate (USD)
	Amount (USD)

	A
	Site Preperation & Earth Work Excavation
	 
	 
	 
	 

	1.1
	Cleaning and removal of trees/shrubs
	LS
	1
	 
	0

	1.2
	Earth work excavation of ash pit (length 2.5m x width 1.5m x depth 1.5m)
	m³
	24
	 
	0

	1.3
	Extra-over for excavation in rock
	m³
	1
	 
	0

	1.4
	Remove surplus excavated material from site and backfill around foundation
	m³
	4
	 
	0

	 
	Total Carried
	 
	 
	 
	 $         -   

	B
	Ash Pit Walls Construction and Concrete Slabs
	 
	 
	 
	 

	2.1
	Construct and install ash pit walls lining with stone masonry to prevent the walls from collapsing  (length 2.5m x width 1.5m x depth 1.5m)
	m³
	26
	 
	0

	2.2
	Construct and install concrete slab at the basement of the ash pit to avoid leaching at the groundwater (length 2.5m x width 1m x breadth 0.2m)
	m³
	4
	 
	0

	2.3
	Construct and install concrete water-tight  cover slab at the top of the pit above the ground to avoid flood runoff water (length 2.2m x width 0.8m x breadth 0.1m), leaving space for the concrete cover lid (0.6m x 0.4m)
	m³
	6
	 
	0

	2.4
	Construct and install concrete cover lid (06m x 0.4m x 0.1m)
	m²
	1
	 
	0

	 
	Total Carried
	 
	 
	 
	 $         -   

	 
	Total for Construction one sharp Pit
	1
	 
	 
	 $         -   

	 
	Fencing of the Entrire Waste Management Zone
	 
	 
	 
	 

	Item
	Description
	Unit 
	Quantity
	Rate (USD)
	Amount (USD)

	 
	Supply and installation of  perimeter wall fencing with masonery basement of 0.6m height with build of wiremesh fencing superstructure 2m height x width 10m x length 10m to protect the entire Waste management zone
	m²
	80
	 
	 $         -   

	 
	Routine maintenance for HCs waste management zone during the project period
	LS
	1
	 
	 $         -   

	 
	Total Fencing of the Entrire waste management zone for continuation of services
	 
	 
	 
	 $         -   

	 
	 
	 
	 
	 
	 

	 
	Summary Total Cost
	 
	 
	 
	 

	 
	Total Construction of Incinerator 
	 
	 
	 
	 

	 
	Total for Placenta Pits for HC
	 
	 
	 
	 

	 
	Total for Construction Ash Pit
	 
	 
	 
	 

	 
	Total for Construction sharp Pit
	 
	 
	 
	 

	 
	Total Fencing of the Entrire Waste Management Zone
	 
	 
	 
	 

	 
	Main total for HCs Incinerators & Fencing waste Management Area
	 
	 
	 
	$0.00

	 
	Main total for TWO HCs Incinerators & Fencing waste Management Area
	 
	 
	 
	$0.00

	 
	Borehole pipeline extension for 2 HC
	 
	 
	 
	 

	 
	Description
	Unit
	Quantity
	Unit cost ($)
	Amount ($)

	 
	Borehole pipeline extension 
	 
	 
	 
	 

	 
	Site preperations and removal of trees and shrubs
	LMS
	1
	 
	 $         -   

	 
	Excavate and install water pipeline pit with dimensions (length 500M x depth 1M x width 0.5M) from main Borehole to the HCs and backfilling of excavated materials after pipeline installation for the two HC
	M³
	1000
	 
	 $         -   

	 
	Install PVC pipe 500M length and diameter of 4 inchs plus other joint fittings
	LMS
	1
	 
	 $         -   

	 
	extention of pipeline to the the departments and Handwashing stations
	LMS
	1
	 
	 $         -   

	 
	Total cost for pipeline extensin for one HC
	 
	 
	 
	 $         -   

	 
	 
	 
	 
	 
	 

	BILL OF QUANTITIES (BOQ) – STONE MASONRY FENCING WALL (20*2.5m)

	Item No
	DESCRIPTION
	UNIT
	QUANTITY
	RATE (USD)
	AMOUNT (USD)

	 
	STONE MASONRY FENCING WALL
	 
	 
	 
	 

	 
	Stone masonry wall, 20 m length × 2.5 m height (50 m²), including cement-sand mortar including basement beam and foundation (0.5m) and Painting
	 
	 
	 
	 

	1
	Stone for masonry wall
	Truck
	34.00
	 
	$0.00

	2
	Clay/soil for construction
	Truck
	15.00
	 
	$0.00

	3
	Cement
	Bag
	150.00
	 
	$0.00

	4
	Sand
	Truck
	10.00
	 
	$0.00

	5
	Iron gate / Ganjeel metal work
	No.
	1.00
	 
	$0.00

	6
	Masonry / wall constructionGate fabrication and installation labour
	Lump sum
	1.00
	 
	$0.00

	 
	GRAND TOTAL
	 
	 
	 
	$0.00

	 
	 
	 
	 
	 
	 

	 
	Total Budget for WASH in Health Facility
	 
	 $         -   




Submission Procedures:
Offers must be received before the deadline which is on 24th Oct 2026 at 12:00 PM hours.
Completed tender documents clearly marked with the EOI Number bided for must be deposited at the NODO Garowe Office before the deadline date and time, and recorded in the log book/ letter.
Formal bids being submitted must be on formal company letters, duly signed and stamped must indicate the Full Company Name, Physical Address, Contact Telephone Number/contact Email address, Directors Names, addresses and their telephone numbers.

Pre-requisites for eligibility are as follows:
To be eligible for participation in this tender procedure, tenderers must prove to the satisfaction of the Contracting Authority that they comply with the necessary legal, technical and financial requirements and have the wherewithal to carry out the contract effectively. Technical and financial submissions must be very explicit. Interested Experienced contractor are invited apply this opportunity.
EVALUATION CRITERIA
Mandatory Requirements
1. Provide a certified copy of a certificate of business registration, certificate of incorporation, business license or similar document. Only vendors within the project areas will be considered.
2. Provide a certified copy of tax registration, tax clearance certificates or similar documents.
3. Quotation/Price list of the items (venders own quotation).
4. Provide information on ownership structure (Name of directors of the company / Owner/shareholders of the business-Contact address including Telephone Number and Passport)
5. Past Experience-Provide references of the previous works or goods supplied before (attach Recommendation letter or Previous Agreements
6. Submit the profile of the trader/business
7. Please indicate Service delivery period
8. Bank Statement For last 12 month and Bank Account Details 
Technical Evaluation
Bids technical evaluation based on the specification submitted
· Further Information to bidders:
Currency of offer should be strictly in US Dollars
NODO does not undertake to pay in advance of work.
NODO reserves the right to accept or reject any offer before the award of a contract, or to cancel the bidding process and reject all offers at any time and is not bound to give reasons for its decisions. Canvassing or giving false information will lead to automatic disqualification.
Incomplete offers or offers which do not comply with any of our tender conditions will not be considered. Quotations should remain valid for a period of at least 90 calendar days after closure of the tender.
It is the Agency’s policy to keep all tender values in confidence.
· Payment:
Upon contracting for works, NODO will pay the contractors in instalments as will be defined in the signed contracts.
· Financial Evaluation
Based on cost quoted
Quotations should be received at NODO Garowe Office behind Kallis Cafeteria. 

Not later than 23th/10/2026 at 12:00 PM.
This EoI does not guarantee a contract of any nature. All proposals will be reviewed and only vendor that meet the required criteria above will receive more details and an invitation to enter into an agreement.
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